#
# Duinomite-eMega board
# =====================
#
# Console on USB
# For Windows, use the driver: http://www.schmalzhaus.com/UBW32/FW/UBW32inf.zip

core pic32mx7
mapping generic
linker bootloader-maximite

device kernel cpu_khz=80000 bus_khz=40000 led=B15

device console device=ttyUSB0
device uartusb

device rdisk led=C1
device sd0 port=3 cs=G12 power=G13

device gpio
