#
# UBW32 board
# ===========
#
# Console on UART2

core pic32mx7
linker bootloader-sdram
mapping generic

device kernel invled=B10
device console invled=B11 device=tty1
device uart2
device rdisk invled=B9 invswap=B8
device sd0 port=2 cs=A9
device sdramp

option PARTITION=sdramp0:sa@2048,fs@14000
