

core pic32mx7
linker bootloader
mapping generic

device kernel cpu_khz=80000 bus_khz=80000 led=D2

device console device=ttyUSB0 led=D0
device uartusb

device rdisk led=D1
device sd0 port=1 cs=A9

device gpio

#device adc
