#
# Fubarino board
# ==============
#
# Console on USB
# SD/MMC card driver on SPI2

core pic32mx7
mapping fubarino
linker bootloader-max32

device kernel led=21 cpu_khz=80000 bus_khz=80000

device console device=ttyUSB0
device uartusb

device sd0 port=2 cs=SS

device gpio
device pwm
device spi
device adc
device glcd
