#
# PONTECH Quick240
# =================
# Console on USB.
# For details, see https://github.com/RetroBSD/retrobsd/wiki/Board-Quick240
#
# To build the kernel, use:
#   cd sys/pic32/pontech_quick240
#   kconfig Config
#   make clean
#   make
#
# Format of this file is described on page:
# http://retrobsd.org/wiki/doku.php/doc/kconfig
#
architecture    "pic32"
cpu             "PIC32MX7"                  # Processor variant
board           "QUICK240"                  # Board type
ldscript        "max32/bootloader.ld"       # Linker script

# Standard system options
options         "CPU_KHZ=80000"             # Oscillator frequency of CPU core
options         "BUS_KHZ=80000"             # Frequency of peripheral bus
options         "BUS_DIV=1"                 # Bus clock divisor 1/2/4/8
options         "USB_AUTOBOOT=YES"          # Don't wait for a keypress on boot

# LED
signal          "LED_KERNEL"    pin RE0     # kernel activity indicator
signal          "LED_DISK"      pin RA7     # kernel activity indicator

# Button
# Hold this button pressed at startup to enter single-user mode.
#signal          "BUTTON1"   pin RG15 invert  # PRG button, active low

# Root filesystem at /dev/sd0a, swap at /dev/sd0b
config          unix    root on sd0a
                        swap on sd0b

# Console options
options         "CONS_MAJOR=UARTUSB_MAJOR"  # UARTUSB device

# Virtual UART on USB
device          uartusb
options         "USB_MAX_EP_NUMBER=3"
options         "USB_NUM_STRING_DESCRIPTORS=3"

# UART ports
device          uart1 
device          uart2 
device          uart3

# SPI ports
controller      spi1                        # SD card

# microSD card
device          sd0     at spi1 pin RD2     # select pin

# General purpose I/O ports
#                                                   1111 11
# Flags define a mask of available pins             5432 1098 7654 3210
device          gpio0   flags 0xc201    # port A    11.. ..1. .... ...1
device          gpio1   flags 0x471f    # port B    .1.. .111 ...1 1111
device          gpio2   flags 0x000e    # port C    .... .... .... 111.
device          gpio3   flags 0x303a    # port D    ..11 .... ..11 1.1.
device          gpio4   flags 0x01fc    # port E    .... ...1 1111 11..
#device          gpio5   flags 0x0000    # port F    .... .... .... ....
device          gpio6   flags 0x70c3    # port G    .111 .... 11.. ..11

# ADC driver
device          adc

# PWM driver
device          pwm
