#
# General dialer definitions used below
#
local|Local PTY connection:\
    :dv=/dev/ptyp0,/dev/ptyp1,/dev/ptyp2,/dev/ptyp3:\
    :br#115200:

dial1200|1200 Baud Able Quadracall attributes:\
	:dv=/dev/cul1:br#1200:cu=/dev/cua1:at=dn11:du:
dial300|300 Bizcomp 1022 attributes:\
	:dv=/dev/cul0:br#300:cu=/dev/cua0:at=dn11:du:
#
# UNIX system definitions
#
unix1200|1200 Baud dial-out to another UNIX system:\
	:el=^U^C^R^O^D^S^Q:ie=%$:oe=^D:tc=dial1200:
unix300|300 Baud dial-out to another UNIX system:\
	:el=^U^C^R^O^D^S^Q:ie=%$:oe=^D:tc=dial300:
#
# System descriptions
#
45|Sytek PDP-11/45:dv=/dev/ttyh1:br#9600:hw:el=^U^C^R^O^D^S^Q:ie=%$:oe=^D:

bert|CSRG ARPA VAX-11/780:pn=@:tc=unix1200:
ernie|UCB VAX-11/780:pn=@:tc=unix1200:
lbl|LBL VAX-11/780:pn=@:tc=unix1200:
decvax|DEC VAX-11/780:pn=@:tc=unix1200:

casevax|cwrunix|CWRU VAX-11/750:pn=@:tc=unix1200:
cwruecmp|ecmp|CWRU VAX-11/780:pn=@:tc=unix1200:
case|CWRU DEC-20:pn=@:tc=unix1200:

ames|Ames TIP:pn=@:tc=unix1200:
navy|navy PWB 11/70:pn=@:tc=unix300:

gi750|General Instruments VAX-11/750, Arizona:pn=@:tc=unix1200:
gi|General Instruments VAX-11/780, Utah:pn=@:tc=unix1200:

video:dv=/dev/tty04:br#4800:




Second example:

45z|PDP-11/45Z system:\
	:dv=/dev/tty32:br#9600:el=^U^C^S^Q^D:ie=%$:oe=^D:
decvax|DEC VAX-11/780:\
	:pn=41148:tc=UNIX-300:
decvax-1200|DEC VAX-11/780:\
	:pn=41230:tc=UNIX-1200:
decmail:\
	:pn=42311:tc=VMS-1200:
ems:\
	:pn=41991:tc=VMS-1200:
vms750|nymph|NPG 750:\
	:dv=/dev/tty36,/dev/tty37:br#9600:el=^Z^U^C^S^Q^O:ie=$@:oe=^Z:
spa|SPA VAX-11/780:\
	:pn=8=2270513:tc=UNIX-300:
vax4|DECnet hub:\
	:pn=41662:tc=VMS-1200:
star|VMS development system:\
	:pn=41701:tc=VMS-1200:
sultan|Software Tools:\
	:pn=41701:tc=UNIX-1200:
cghub|demo room timesharing VAX:\
	:pn=41023,41024:tc=VMS-300
phenix|phenix-300|Distributed systems:\
	:pn=8=2472765,8=2472766,8=2472767,8=2472768:tc=VMS-300
market|arpanet:\
	:pn=8=2317437,8=2317438,8=2317447,8=2317447,8=2317448,8=2317449,\
	:8=2317450,8=2317451:tc=TOPS20-1200
market300|arpanet300:\
	:pn=8=2311120,8=2311125,8=2311128:tc=TOPS20-300
tip0|tip1200:tc=UNIX-1200:
tip300:tc=UNIX-300:
cu0|cu300:tc=UNIX-300:
cu1200:tc=UNIX-1200:
UNIX-300:\
	:dv=/dev/cua0:el=^D^U^C^S^Q^O@:du:at=df02:ie=#$%:oe=^D:br#300:
UNIX-1200:\
	:dv=/dev/cua1,/dev/cua2,/dev/cua4:el=^D^U^C^S^Q^O@:du:at=df03:\
	:ie=#$%:oe=^D:br#1200:
VMS-300|TOPS20-300:\
	:dv=/dev/cua0:el=^Z^U^C^S^Q^O:du:at=df02:ie=$@:oe=^Z:br#300:
VMS-1200|TOPS20-1200:\
	:dv=/dev/cua1,/dev/cua2,/dev/cua4:el=^Z^U^C^S^Q^O:du:at=df03:\
	:ie=$@:oe=^Z:br#1200:
--------------------------------------------------------------------
The attributes are:

dv	device to use for the tty
el	EOL marks (default is NULL)
du	make a call flag (dial up)
pn	phone numbers (@ =>'s search phones file; possibly taken from
			      PHONES environment variable)
at	ACU type
ie	input EOF marks	(default is NULL)
oe	output EOF string (default is NULL)
cu	call unit (default is dv)
br	baud rate (defaults to 300)
fs	frame size (default is BUFSIZ) -- used in buffering writes
	  on receive operations
tc	to continue a capability
