#
# Explorer16 board
# ================
#

core pic32mx7
linker bare
mapping generic

device kernel cpu_khz=80000 bus_khz=80000 led=A1

device console led=A2 device=tty1
device uart2 baud=115200

device rdisk led=A0 swap=A3
device sd0 port=1 cs=B1 mhz=10

device gpio
