#
# MikroElektronika MMB for PIC32MX7 board
# =======================================
#
# Console on USB
# For Windows, use the driver: http://www.schmalzhaus.com/UBW32/FW/UBW32inf.zip

core pic32mx7
linker bootloader
mapping generic

device kernel invled=A0 clear_pin=D2
device console invled=A1 device=ttyUSB0
device uartusb
device rdisk invswap=D9
device sd0 port=1 cs=A9 mhz=8
device gpio
device adc
device uart1
